|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Table 3. Comparison of reference evapotranspiration ETo from MOD16 and towers. Numbers in parenthesis indicate the error % between ETo from MOD16 and ETo from the tower. | | | | |
| Tower | Year | ETo Tower | ETo MOD16 | |
|  |  | mm/day | mm/day | Error |
| StaD | 2012 | 6.3 | 6.1 | -3% |
| StaW | 2012 | 6.3 | 6.1 | -3 |
| Wil | 2012 | 5.4 | 6.2 | +15 |
| Big | 2011 | 5.4 | 5.7 | +6 |
| Fiv | 2011 | 6.4 | 6.9 | +8 |
| Mean |  | 6.0 | 6.2 | +5 |

plot\_ts\_PET\_MOD16\_tower\_multiple\_in\_one.R